Da Gong gongda@jlu.edu.cn

Subglacial drilling and sampling

Poster

STUDY ON SEDIMENT CORING TECHNIQUES IN ANTARCTIC SUBGLACIAL WATER ENVIRONMENT

|  |  |
| --- | --- |
| Da Gong1, Xiaopeng Fan1, Yazhou Li2, Bing Li2, Pavel Talalay1,2, Nan Zhang1, Ziyan Wu1, Ximu Liu1, Zhipeng Deng1, Xianzhe Wei1, Yuan Wang1, Ting Wang1 | 1Polar Research Center, Institute for Polar Science and Engineering, Jilin University, Changchun, China  2China University of Geosciences, Beijing, China |

Antarctic subglacial sediments preserve important geological and ecological records, including paleoenvironmental changes, glacier melting processes, and subglacial ecosystem dynamics. However, current coring technology is difficult to cope with heterogeneous formation sediments containing hard particles (such as gravel, granite pebbles) and viscous clay matrix, which have high shear strength (2-22kPa). This study focuses on developing advanced sediment coring techniques for complex structural formations in the Antarctic ice water environment, aiming to address key challenges such as insufficient penetration depth (<3m), severe sample interference, and difficulty in recovery in existing sampling methods. This study employed multiple methods: Studies include: (1) reconstructing subglacial sedimentary layers through laboratory simulations, incorporating mineral composition and particle size distribution based on actual samples; (2) using energy dissipation models to study the infiltration mechanism under impact loads, in order to analyze crack propagation in hard particles and stress response in clay layers; (3) develop low interference sampling technology with innovative tool design to minimize interference with the water sediment interface layer; (4) Research on reducing the pulling force of sampling tubes through pressure compensation and core tube structural optimization. The penetration mode mainly focus on hammering and vibration sampling, which are expected to achieve deeper footage in these complex sedimentary formations. Laboratory coring tests, load analysis, and sample recovery were also studied through relevant experiments. These results will provide technical support for sediment sampling under the Antarctic ice shelf, glacial lakes, and subglacial lakes.

References

[1] Dominic A. Hodgson, Michael J. Bentley, James A. Smith, Julian Klepacki, Keith Makinson, Andrew M. Smith, Kevin Saw, Reed Scherer, Ross Powell, Slawek Tulaczyk, Mike Rose, David Pearce, Matt Mowlem, Peter Keen and Martin J. Siegert, Technologies for retrieving sediment cores in Antarctic subglacial settings, Philosophical Transactions of the Royal Society A: Mathematical, Physical and Engineering Sciences, vol. 374, no. 2059, Jan. 2016. <https://doi.org/10.1098/rsta.2015.0056>

[2] Da Gong, Xiaopeng Fan, Yazhou Li, Bing Li, Nan Zhang, Raphael Gromig, Emma C. Smith, Wolf Dummann, Sophie Berger, Olaf Eisen, Jan Tell, Boris K. Biskaborn, Nikola Koglin, Frank Wilhelms, Benjamin Broy, Yunchen Liu, Yang Yang, Xingchen Li, An Liu, Pavel Talalay\*, Coring of Antarctic Subglacial Sediments, Journal of Marine Science and Engineering, 2019, 7(6), 194. <https://doi.org/10.3390/jmse7060194>

[3] Makinson, K., Ashurst, D., Anker, P. G. D., Smith, J. A., Hodgson, D. A., Davis, P. E. D., & Smith, A. M. (2021). A new percussion hammer mechanism for a borehole deployable subglacial sediment corer. Annals of Glaciology, 62(85–86), 385–389. doi:10.1017/aog.2020.83