Liangyu Wang [wlybook@163.com](mailto:wlybook@163.com); znan@jlu.edu.cn

**Hot water drilling**

Oral

STUDY ON THE FORMATION MECHANISM OF DEEP HOT-WATER DRILLING BACKWATER CAVITY

|  |  |
| --- | --- |
| *Liangyu Wang1,* *Nan Zhang1,\*,* *Xiaopeng Fan1, Da Gong1, Wei Wu1, Yifan Yang1,Xu Zhang1, Mingrui Guo1, Ximu Liu1, Zhipeng Deng1, Zejun Liu2* | 1Polar Research Center, Institute for Polar Science and Engineering, Jilin University, Changchun, China  \*Polar Research Center, Institute for Polar Science and Engineering, Jilin University, Changchun, China  2China University of Geosciences, Beijing, China |

For explore and sample subglacial lakes in polar regions, hot-water drilling has emerged as the most rapid and efficient penetration method(P. G. Talalay et al. 2024). In a deep polar hot-water drilling system, the backwater system is an essential component , with the backwater cavity playing a pivotal role( Zhipeng Deng et al. 2025). Located at a specific depth beneath the ice sheet surface, this ice-enclosed void is crucial for storing and recycling water during the drilling process. It also ensures hydraulic equilibrium upon reaching subglacial lakes, thereby enhancing overall drilling efficiency significantly. This study employed scaled-down laboratory model experiments to systematically investigate the formation of backwater cavities under various parameters. The research comprised two initial test series: (1) examining cavity formation using nozzles of different diameters, and (2) analyzing cavity formation with different nozzle divergence angles. These tests identified the optimal nozzle specifications for cavity generation. Subsequently, four sets of experiments were conducted using the selected nozzles, including the formation of backwater cavities with multiple nozzles, the formation of backwater cavities with different hot water temperatures, the formation of backwater cavities at varying flow rates, and the formation of backwater cavities with different nozzle installation angles. By exploring the influence of these parameters on the backwater cavity formation process, the study aimed to determine the parameter settings most suitable for field operations in Antarctica. Based on the experimental findings, the study deduced the appropriate nozzle parameters for Antarctic fieldwork and designed the corresponding nozzle types. The test results indicated that the optimal water spraying speed for backwater cavity formation is 37.23 m/s. For single-row, six-nozzle configurations, fan-shaped nozzles with a diameter of 4.4 mm and a scattering angle of 80° are recommended. In summary, this research provides valuable insights into optimizing the design and operation of hot-water drilling systems for polar exploration, laying a solid foundation for future subglacial lake exploration projects.

References

Talalay PG, Zhang N, Fan X, Li B, Li Y, Yu H, Zuo H, Li L, Shi G, Shi W, Guo M, Yang Y, Wang T, Gong D, Hong J, Li Y (2024) General concept of a deep hot water drilling system and drilling strategy to access Subglacial Lake Qilin, East Antarctica. Arctic and Antarctic Research 70 (Supp):54-64. <https://doi.org/10.30758/0555-2648-2024-70-4-514-524>

Deng, Z., Sun, Y., Fan, X., Talalay, P., Yang, Y., Liu, X., Gong, D., Li, B., Wang, T., Wu, W., Zhang, N., & Wei, X. (2025). Experimental Study on the Hole-Forming Process at the Borehole Bottom During Hot Water Drilling in Ice and Its Influence Mechanisms. Journal of Marine Science and Engineering, 13(4), 817. <https://doi.org/10.3390/jmse13040817>

Talalay, P., Liu, G., Wang, R., Fan, X., Hong, J., Gong, D., Liu, B., Liu, A., & Sysoev, M. (2018). Shallow hot-water ice drill: Estimation of drilling parameters and testing. Cold Regions Science and Technology, 155, 11–19. <https://doi.org/10.1016/j.coldregions.2018.07.006>

Liu, A., Wang, R., Fan, X., Yang, Y., Li, X., Wang, L., & Talalay, P. (2019). Test-Bed Performance of an Ice-Coring Drill Used with a Hot Water Drilling System. *Journal of Marine Science and Engineering*, *7*(7), 234. https://doi.org/10.3390/jmse7070234